2.

(a) They have two inputs S (for set) and R (for reset)

(b) D-latch, present and next state are the same as long as the timing control input is asserted. D flip-flop, next state can only be written into memory on the edge of the timing signal.